Use angular velocity with threshold

Use acceleration considering position

Knn / svm for separation of peaks and lows

Feature extractor – accelerator, gyroscope, angular velocity

Transformation and normalization